# IP Camera

Smartphone-ready colour night/day

network camera with pan, tilt and zoom

# DYN-631



# SPECIFICATIONS:

* Product type: IP camera
* Operation system: Embedded operating system
* Web protocol: TCP/IP, UDP/IP, HTTP, SMTP, FTP, DHCP, DDNS, UPNP, NTP, RTSP, ONVIF
* LAN port: 802.11 b/g/n
* Wifi: 10Base-T/100Base-TX
* Resolution: 720P, 640\*360, 320\*180
* Compression mode: H.264/M-JPEG
* Max frame rate: 30fps
* Lens: f=3.6mm, F=2.0
* Min. illumination: IR on, 0 Lux
* Electronic shutter: 1/50s(1/60s)-1/100,000 s
* SNR: 48db
* Safety performance: Three levels of user rights
* Install mode: Wall-mounted / ceiling-mounted
* Other performance: PC software,support for Microsoft Windows 98/2000/XP/Vista/Windows 7/Mac OS, And the
* Internet Explorer6.1 and above version or browser compatibility, Firefox, etc., provide SmartViewPro client software
* Power supply: DC 5V
* Sensor: CMOS Sensor
* IP camera performance: Support video control, Two-way voice talkback, motion detection, external alarm(sends information to alarm the server by Email, FTP); Manufacturers provide free DDNS, and has been written into equipment; 12pcs IR LEDs,8 meters effectively; Platform level angle 350 °, 90 °vertical angle; automatically control through the photoresistor;
* Audio input: With microphone
* Audio output: Build-in loudspeaker, provide the audio output interface
* Alarm in: Not supported
* Alarm out: Not supported
* Power consumption: Power<6W
* Body size: 105\*116\*126mm
* Product weight: 0.40kg
* Environment temperature: -10℃--50℃℃
* Environment humidity: below 85% RH