# IP Camera

## Smartphone -ready colour night/day

## network camera with pan, tilt and zoom

**DYN-615**



# Specification

Product type：IP camera

Operation system：Embedded operating system

Web protocol：TCP/IP, UDP/IP, HTTP, SMTP, FTP, DHCP, DDNS, UPNP, NTP, RTSP, ONVIF

LAN port：10Base-T/100Base-TX

Wifi：802.11 b/g/n

Resolution：VGA; QVGA; QQVGA

Compression mode：M-JPEG

Max frame rate：30fps

Lens：f=3.6mm, F=2.0

Min. illumination：IR on, 0 Lux

Electronic shutter：1/50s(1/60s)-1/100,000 s

SNR：48db

Safety performance：Three levels of user rights

Install mode：Wall-mounted

Other performance：PC software,support for Microsoft Windows 98/2000/XP/Vista/Windows 7/Mac OS,And the Internet Explorer6.1 and above version or browser compatibility, Firefox, etc., provide iSmartViewPro client software

Power supply：DC 5V

Sensor：CMOS Sensor

IP camera performance：Support video control, Two-way voice talkback, motion detection, external alarm(sends information to alarm the server by Email, FTP); Manufacturers provide free DDNS, and has been written into equipment; 18pcs IR LEDs, up to 15meters night vision; automatically control through the photoresistor;

Audio input：None

Audio output：None

Alarm in：Not supported

Alarm out：Not supported

Power consumption：Power<6W

Body size：153\*96\*96mm

Product weight：0.53kg

Environment temperature：-10℃--50℃℃

Environment humidity：below 85% RH