# IP Camera

**Home/ Office CCTV Surveillance**

**Made Easy**

**DYN-700**



# DESCRIPTION

The exciting DYN-700 Smartphone-ready wireless IP camera is your ideal security partner for home or office. Forget messy, complex setups, the DYN-700 can be setup in just a few minutes from your smartphone, tablet or computer - WindowsTM, MacTM or AndroidTM.

Superb HD colour display, watch in both daylight and total darkness and get an email when

motion is detected, the choice is yours 24/7.

# FEATURES

* HD, Colour CMOS with multi-coated optics
* HD 1-Megapixel capturing with 3.6mm lens
* Instant setup - No messy router setups needed
* HD quality audio with built-in microphone
* Supports up to 720p, 360p and 180p resolutions
* Built-in super fast 802.11n WiFi (b/g supported)
* Motion detection alarm setup
* Supports multi-view display for multiple IP cameras
* Multi- language support with free client software

# SPECIFICATIONS

|  |  |  |
| --- | --- | --- |
| Model | 700GC | |
| Hardware performance | Product type | IP camera |
| Operation system | Embedded operating system |
| Special function | One key WIFI setting, no need network cable |
| Web environment | Web protocol | TCP/IP, UDP/IP, HTTP, SMTP, FTP, DHCP, DDNS, UPNP, NTP, RTSP, ONVIF |
| Wifi | WIFI, 802.11 b/g/n |
| Image performance | Resolution | 720P, 640\*360, 320\*180 |
| Compression mode | H.264/M-JPEG |
| Max frame rate | 30fps |
| Other parameters | Lens | f=3.6mm, F=2.0 |
| Min. illumination |  |
| Electronic shutter | 1/50s(1/60s)-1/100,000 s |
| SNR | 48db |
| Safety performance | Three levels of user rights |
| Install mode | Wall-mounted / ceiling-mounted |
| Other performance | PC software,support for Microsoft Windows 98/2000/XP/Vista/Windows 7/Mac OS,And the Internet Explorer6.1 and above version or browser compatibility, Firefox, etc., provide iSmartViewPro client software |
| Power supply | DC 5V |
| Sensor | 1/4’’ CMOS Sensor |
| IP camera performance | Support video control, motion detection, external alarm(sends information to alarm the server by Email, FTP); |
| Audio input | With microphone |
| Audio output | Not supported |
| Alarm in | Not supported |
| Alarm out | Not supported |
| Power consumption | Power<4W |
| Appearance parameters | Body size | 66\*44.5\*76.5mm |
| Product weight | 0.104kg |
| Environment parameters | Environment temperature | -10℃-50℃ |
| Environment humidity | below 85% RH |

**Packing List**

* 1, IP Camera\* 1
* 2, Quick installation Guide\* 1
* 3, Power Adapter \*1
* 4, Screw\*1kit
* 5, Certificate of qualification\*1