### 10 Way Vertically Mounted Rackmount IEC PDU - UK Sockets (PDU-10WS-V)



# **Description:**

The LMS Power **PDU-10WS-V** is a high-quality vertically mounted PDU (**P**ower **D**istribution **U**nit) that simply fits within the universal horizontal mounting brackets of data, telecom and server cabinets.

A critical accessory for your data cabinets if you need to provide effective power to devices including Ethernet Switches, Servers, UPS, NAS and of course cabinet accessories including cooling fan trays.

Robust, alloy design complete with rackmount brackets fitted, high-quality Neon Switch and of course UK output sockets together with a high quality, BSI-fitted
13 Amp UK plug.

# **Key Features:**

Standard UK 3-Pin power outlets for your appliances

Certified IEC-14 power input plug

1U vertically mounted attaches to internal profiles

Neon On/Off Rocker switch to prevent accidental turn off

Backed up by LMS Power's exclusive 3-year warranty

# **Applications:**

Create instant power feeds to your data, telecom or server cabinets

Provide effective power for cabinet cooling fans, UPS systems

Ideal as stand-alone trailing sockets outside the cabinet

# **Product Code:**

Part Number: PDU-10WS-V-UK-IEC

EAN: 8400800036124

Weight: 1.5Kg approx

# **Technical Specifications:**

Warranty                 LMS Data 3-Year Warranty

Chassis                   1U vertical PDU with mounting brackets

Output Sockets      10 UK 3-PIN Sockets

Power Input            Fitted IEC-14 Plug

Flex Length             1.8 metres (approx)

Power Control        On/Off Rocker Switch (illuminated)

Power Rating          4000 Watts (approx)

# **Supplied With:**

PDU-6WS-H-UK-IEC  10 Way Vertical PDU

Cabinet brackets (Fitted)

*\* Specifications and product design are subject to change. E&OE.*

Need a competitively priced but quality Power Distribution Unit (PDU) for your applications or installation? The new PDU-10WS-V is a robust, non-surged protected PDU which features effective electrical distribution to its integral, 10-way, UK-socketed 3-pin sockets. Combining a fully certified UK plug input combined with a compatible heavy load power flex means you can be assured this LMS Data PDU can work without problems, 24/7. Ideal for data, telco and broadcast applications, with the added benefit of a low-profile, 1U hight and the ability to be mounted vertically in almost all floor, telco and server enclosures via the standard mount slots. Robust in design, with an integral neon illuminated rocker switch for assured functionality, the LMS Data PDU is designed to deliver maximum electrical power - today and tomorrow.

# **specifications:**

Vertical, high-density Power Distribution Unit (PDU)

UK-plug style plug power input

10-Way UK, 3-Pin Power Outlets

Robust, black aluminium design for industrial use

Neon on/off power switch for assured control

Maximum power rating - 4000W (approx.)

1.8 metre (approx.) power cordage

Ideal for data, telecom, broadcast and HVAC applications