### 12 Way Horizontally Mounted Rackmount IEC 20 Plug PDU - IEC 13 Sockets (PDU-12WS-H-IEC-IEC20)



# **Description:**

The LMS Power**PDU-12WS-H-IEC-IEC20**is a high-quality horizontally mounted PDU (**P**ower **D**istribution **U**nit) that simply fits within the universal mounting brackets of data, telecom and server cabinets.

A must-have accessory for your data cabinets if you need to provide effective power to devices including Ethernet Switches, Servers, UPS, NAS and of course cabinet accessories including cooling fan trays.

Robust, alloy design complete with rackmount brackets fitted, high-quality Neon Switch, standardised IEC 13 power outlets, the PDU being fitted with a standardised IEC 20 Plug.

# **Key Features:**

Standard IEC 13 power outlets for your appliances

Standardised IEC 20 power plug

1U horizontally mounted attaches to internal profiles

Neon On/Off Rocker switch to prevent accidental turn off

Backed up by LMS Power's exclusive 3-year warranty

# **Applications:**

# Create instant power feeds to your data, telecom or server cabinets

# Provide effective power for cabinet cooling fans, UPS systems

# Ideal as stand-alone trailing sockets outside the cabinet

# **Product Code:**

Part Number: PDU-12WS-H-IEC-IEC20

EAN: 8400800030702

Weight: 1.7Kg approx

# **Technical Specifications:**

Warranty                 LMS Data 3-Year Warranty

Chassis                    1U horizontally PDU with mounting brackets

Output Sockets     12 IEC 13 Sockets

Power Input            Standardised IEC 20 Plug

Flex Length             2 metres (approx)

Power Control        On/Off Rocker Switch (illuminated)

Power Rating          4000 Watts (approx) Surge Protected

# **Supplied With:**

PDU-12WS-H-IEC-IEC20    12 Way Horizontal PDU

Cabinet brackets (Fitted)

*\* Specifications and product design are subject to change. E&OE.*

Looking for a more specialised, higher density Power Distribution Unit (PDU) to provide power to a wide variety of devices? The new LMS Data PDU-12WS-H-IEC-IEC20 is a high-density, horizontal placement PDU which features 12 standard IEC-C13 socketed outlets to provide power to networking, data centre, PBX and broadcast level power devices within the data cabinet enclosure. Horizontal placement within almost any type of 19-inch wide wall, telco or server enclosure is assured thanks to its universal design together with a host of mounting options within the enclosure. Coupled with a long-life, illuminated I/O Switch, certified power sockets together with a generous length power cord to the attached IEC-C20 power input plug.

# **specifications:**

12-way IEC-C13 Socket Power Distribution Unit (PDU)

Compliant, IEC-C20 power input plug

Illumination On/Off power-input rocker switch

Integral Grounding built into the chassis

Generous length, 1.8 metre (approx.) power cable

Lightweight, horizontal design with mount brackets

Ideal for horizontal placement in data or server enclosures

Ideal for LAN, audio-visual, PBX, VoIP and CCTV applications