### 8 Way Vertically Mounted Surge Protected Rackmount PDU - UK Sockets (PDU-8WS-V-SP-1U)

### 

# **Description:**

# The LMS Power **PDU-8WS-V-SP-1U** is a high-quality surge protected, vertically mounted PDU (**P**ower **D**istribution **U**nit) that simply fits within the universal mounting brackets of data, telecom and server cabinets.  Providing piece-of-mind of integral electrical surge protection against common power surges and electrical spikes to devices including Ethernet Switches, Servers, UPS, NAS and of course cabinet accessories including cooling fan trays. Robust, alloy design complete with rackmount brackets fitted, high-quality Neon Switch and of course UK output sockets together with a high quality, BSI-fitted 13 Amp UK plug.

# **Key Features:**

Standard UK 3-Pin power outlets for your appliances  
  
Built-in surge protection for critical device protection  
  
1U vertically mounted attaches to internal profiles  
  
Neon On/Off Rocker switch to prevent accidental turn off   
  
Backed up by LMS Power's exclusive 3-year warranty

# **Product Code:**

Part Number: PDU-8WS-V-SP-1U  
  
EAN: 8400800024251

Weight: 1.5Kg approx

# **Technical Specifications:**

Warranty                 LMS Data 3-Year Warranty  
                         
Chassis                   1U vertical PDU with mounting brackets   
  
Output Sockets       8 UK 3-PIN Sockets

Power Input            Fitted UK 3PIN BSI Plug 13 Amp  
  
Flex Length             1.8 metres (approx)  
  
Power Control        On/Off Rocker Switch (illuminated)  
  
Power Rating          4000 Watts (approx) Surge Protected

# **Supplied With:**

PDU-8WS-V-SP-1U  8 Way Vertical PDU  
  
Cabinet brackets (Fitted)  
*\* Specifications and product design are subject to change. E&OE.*

Looking for a more specialised Power Distribution Unit (PDU) with integral surge protection and grounding validation features? The new LMS Data PDU-8WS-V-SP-1U is a high-density, vertical placement PDU which features 8 standard UK power socket outlets to provide power to networking, data centre, PBX and broadcast level power devices within the data cabinet enclosure. Integral status LED for electrical earthing indication is an important safety feature, reducing the risk of electric shock for both the attached devices and of course installation staff. Surge protection is of course built-in to all outlet sockets, increasing both MTBF and reduced data corruption for attached computing and networking devices. Coupled with a long-life, illuminated I/O Switch, certified UK power sockets together with a generous length power cord, all of which are BSI rated and fused for full compliance.

# **specifications:**

8-way UK plug-socket style Power Distribution Unit (PDU)

Compliant, 13-amp UK 3-pin socket output

Illumination On/Off power-input rocker switch

Integral Surge Protection and Grounding Confirmation

Generous length, 1.8 metre (approx.) power cable

Lightweight design with a 1U high form-factor design

Ideal for vertical placement in data or server enclosures

Ideal for LAN, audio-visual, PBX, VoIP and CCTV applications