# 12 Way Vertically Mounted Rackmount PDU - UK Sockets (PDU-12WS-V)



**PDU-12WS-V**

# DESCRIPTION

The LMS Power **PDU-12WS-V** is a high-quality vertically mounted PDU (**P**ower **D**istribution **U**nit) that simply fits within the universal horizontal mounting brackets of data, telecom and server cabinets.

A critical accessory for your data cabinets if you need to provide effective power to devices including Ethernet Switches, Servers, UPS, NAS and of course cabinet accessories including cooling fan trays.

Robust, alloy design complete with rackmount brackets fitted, high-quality Neon Switch and of course UK output sockets together with a high quality, BSI-fitted

13 Amp UK plug.



# ****Key Features****:

**Standard UK 3-Pin power outlets for your appliances**

**1U vertically mounted attaches to internal profiles**

**Neon On/Off Rocker switch to prevent accidental turn off**

**Backed up by LMS Power's exclusive 3-year warranty**

# SPECIFICATIONS

Warranty                 LMS Data 3-Year Warranty

Chassis                   1U vertical PDU with mounting brackets

Output Sockets      12 UK 3-PIN Sockets

Power Input            Fitted UK 3PIN BSI Plug 13 Amp

Flex Length             1.8 metres (approx)

Power Control        On/Off Rocker Switch (illuminated)

Power Rating          4000 Watts (approx)

# Applications:



Create instant power feeds to your data, telecom or server cabinets

Provide effective power for cabinet cooling fans, UPS systems

Ideal as stand-alone trailing sockets outside the cabinet

# Product Code:

Part Number: PDU-12WS-V

EAN: 8400800035110

Weight: 1.7Kg approx

# Supplied With:

PDU-12WS-V   12 Way Horizontal PDU

Cabinet brackets (Fitted)

\* Specifications and product design are subject to change. E&OE.