### 6 Way Horizontally Mounted Rackmount UK Plug PDU - IEC 13 Sockets (PDU-6WS-H-IEC-UK)

### 

# **Description:**

The LMS Power **PDU-6WS-H-IEC-UK**is a high-quality horizontally mounted PDU (**P**ower **D**istribution **U**nit) that simply fits within the universal mounting brackets of data, telecom and server cabinets.   
  
A critical accessory for your data cabinets if you need to provide effective power to devices including Ethernet Switches, Servers, UPS, NAS and of course cabinet accessories including cooling fan trays.

Robust, alloy design complete with rackmount brackets fitted, high-quality Neon Switch, standardised IEC 13 power outlets, the PDU being fitted with a BSI rated, 13 Amp UK plug.

# **Key Features:**

Standard IEC 13 power outlets for your appliances  
  
Certified BSI 13-Amp UK fitted plug  
  
1U horizontally mounted attaches to internal profiles  
  
Neon On/Off Rocker switch to prevent accidental turn off   
  
Backed up by LMS Power's exclusive 3-year warranty

# **Applications:**

Create instant power feeds to your data, telecom or server cabinets  
  
Provide effective power for cabinet cooling fans, UPS systems  
  
Ideal as stand-alone trailing sockets outside the cabinet

# **Product Code:**

Part Number: PDU-6WS-H-IEC-UK

EAN: 8400800026118

Weight: 1.2Kg approx

# **Technical Specifications:**

Warranty                 LMS Data 3-Year Warranty  
                         
Chassis                   1U horizontally PDU with mounting brackets   
  
Output Sockets      6 IEC 13 Sockets

Power Input            Fitted BSI 13 AMP UK Plug  
  
Flex Length             2 metres (approx)  
  
Power Control        On/Off Rocker Switch (illuminated)  
  
Power Rating          4000 Watts (approx) Surge Protected

# **Supplied With:**

PDU-6WS-H-IEC-UK  6 Way Horizontal PDU  
  
Cabinet brackets (Fitted)  
*\* Specifications and product design are subject to change. E&OE.*