### 6 Way Horizontally Mounted Surge Protected Rackmount IEC PDU - UK Sockets (PDU-6WS-H-SP-1U-IEC)

###

# **Description:**

# The LMS Power **PDU-6WS-H-SP-1U-IEC**is a high-quality surge protected, horizontally mounted PDU (**P**ower **D**istribution **U**nit) that simply fits within the universal mounting brackets of data, telecom and server cabinets. Providing piece-of-mind of integral electrical surge protection against common power surges and electrical spikes to devices including Ethernet Switches, Servers, UPS, NAS and of course cabinet accessories including cooling fan trays.Robust, alloy design complete with rackmount brackets fitted, high-quality Neon Switch and of course UK output sockets together with a high quality, BSI-fitted13 Amp UK plug.

# **Key Features:**

**Standard UK 3-Pin power outlets for your appliances

Built-in surge protection for critical device protection**
**1U horizontally mounted attaches to internal profiles**

**Neon On/Off Rocker switch to prevent accidental turn off**

**Backed up by LMS Power's exclusive 3-year warranty**

# **Product Code:**

Part Number: PDU-6WS-H-SP-1U-IEC

EAN: 8400800020499

Weight: 1.2Kg approx

# **Technical Specifications:**

Warranty                 LMS Data 3-Year Warranty

Chassis                   1U horizontally PDU with mounting brackets

Output Sockets      6 UK 3-PIN Sockets

Power Input            Fitted UK 3PIN BSI Plug 13 Amp

Flex Length             1.8 metres (approx)

Power Control        On/Off Rocker Switch (illuminated)

Power Rating          4000 Watts (approx) Surge Protected

# **Supplied With:**

PDU-6WS-H-SP-1U-IEC   6 Way Horizontal PDU

Cabinet brackets (Fitted
*\* Specifications and product design are subject to change. E&OE.*

Looking for highperformance power distribution for your heavily loaded systems? The newly developed LMS Data 13A heavy-duty horizontal PDU using the IEC-14 plug input connector which is ideal for many device requirements including server, network and other industrial-type equipment functions such as broadcast and HVAC applications. Combining a fully certified IEC-14 plug input combined with a compatible heavy load power flex means you can be assured this LMS Data PDU can work without problems, 24/7. Furthermore, incorporated onto the horizontal form-factor are industry standard UK sockets, ideal for data, telco and broadcast equipment with the added benefit of integral electrical surge protection. Robust in design, with an integral neon illuminated rocker switch for assured functionality, the LMS Data PDU is designed to deliver maximum electrical power today and tomorrow.

# **specifications:**

Horizontal Power Distribution Unit (PDU)

Certified IEC-14 power input plug

Compatible, heavy-load power cable

6x UK power sockets

Robust, black aluminium design for industrial use

Neon on/off power switch for assured control

Maximum power rating - 4000W

2.0 metre (approx.) power cordage

Ideal for data, telecom, broadcast and HVAC applications