### 6 Way Horizontally Mounted Rackmount IEC PDU 3M - UK Sockets (PDU-6WS-H-UK-IEC-3M)

### 

# **Description:**

The LMS Power **PDU-6WS-H-UK-IEC-3M**is a high-quality horizontally mounted PDU (**P**ower **D**istribution **U**nit) that simply fits within the universal mounting brackets of data, telecom and server cabinets.   
  
A must-have accessory for your data cabinets if you need to provide effective power to devices including Ethernet Switches, Servers, UPS, NAS and of course cabinet accessories including cooling fan trays.

Robust, alloy design complete with rackmount brackets fitted, high-quality Neon Switch and of course UK output sockets together with a high quality, certified  
IEC-14 power input plug.

# **Key Features:**

Standard UK 3-Pin power outlets for your appliances  
  
Extra long 3m Power Flex for difficult installs  
   
Certified IEC-14 power input plug  
  
1U horizontally mounted attaches to internal profiles  
  
Neon On/Off Rocker switch to prevent accidental turn off   
  
Backed up by LMS Power's exclusive 3-year warranty

# **Product Code:**

Part Number: PDU-6WS-H-SP-UK-IEC-3M

EAN: 8400800032676

Weight: 1.2Kg approx

# **Technical Specifications:**

Warranty                 LMS Data 3-Year Warranty  
                         
Chassis                  1U horizontally PDU with mounting brackets   
  
Output Sockets      6 UK 3-PIN Sockets

Power Input            Fitted IEC-14 Plug  
  
Flex Length             3 metres (approx)  
  
Power Control        On/Off Rocker Switch (illuminated)  
  
Power Rating          4000 Watts (approx) Surge Protected

# **Supplied With:**

PDU-6WS-H-SP-UK-IEC-3M  6 Way Horizontal PDU  
  
Cabinet brackets (Fitted)  
*\* Specifications and product design are subject to change. E&OE.*

Looking for highperformance power distribution for your heavily loaded systems? The newly developed LMS Data 13A heavy-duty horizontal PDU using the IEC-14 plug input connector which is ideal for many device requirements including server, network and other industrial-type equipment functions such as broadcast and HVAC applications. Combining a fully certified IEC-14 plug input combined with a compatible heavy load power flex means you can be assured this LMS Data PDU can work without problems, 24/7. Furthermore, incorporated onto the horizontal form-factor are industry standard UK sockets, ideal for data, telco and broadcast equipment with the added benefit of integral electrical surge protection. Robust in design, with an integral neon illuminated rocker switch for assured functionality, the LMS Data PDU is designed to deliver maximum electrical power today and tomorrow.

# **specifications:**

Horizontal Power Distribution Unit (PDU)

Certified IEC-14 power input plug

Compatible, heavy-load power cable

6x UK power sockets

Robust, black aluminium design for industrial use

Neon on/off power switch for assured control

Maximum power rating - 4000W

2.0 metre (approx.) power cordage

Ideal for data, telecom, broadcast and HVAC applications