# 

### 50 Port 2U Rackmount CAT3/TELCO 6-Pin Patch Panel (PPAN-50-T)



# Description:

The LMS Data PPAN-50-T is 50 Port enhanced CAT3 and Telecommunications Patch Panel for working in low bandwidth applications of that of legacy PABX Telco applications.

Fully certified to CAT3/Telco standards allowing typical voice call cables to be terminated and thus patched via the 6-PIN front connection ports.

Long-life, nickel plated female ports are coupled with a vertical designed Krone(tm) IDC terminal IDC together with rear cable management bar and tabs.

# Key Features:

* Certified CAT3/TELCO 50 Way Patch Panel
* Standard 6-Pin Ports with Krone(tm) IDC Punchdown
* 2u High means it fits in the smallest of data cabinets
* Part of the Synthesis 25-Year Warranty Solution

# Specifications

* 48-Port, High-Density 2-U Through Coupler Patch Panel
* Performance Cat5e UTP certified - Gigabit Compliance
* Easy-Clip, modular through coupler design\*
* Meets or Exceeds current Category 5e performance
* Built-in LAN port redundancy - Easy to swap out
* High conductive, gold-plated RJ45 connections
* Individual port numbering (1-48)
* Supplied with x2 clip-on alloy rear cable management bars
* Supplied with standard M6 cage nuts, bolts and washers

# Applications:

* Office, Education and Home Structured Cabling Installs
* Ideal for Gigabit Ethernet (1000Mbps) Data Networks
* Create fault tolerant LANs by simply patching ports

# Product Code:

* Part Number: PPAN-50-T
* EAN: 8400800013286
* Weight: 2 Kg approx.

# Technical Specifications:

* Port Count：50 Ports UTP
* Dimensions：2U 19-Inch Design Format
* Design：6-Pin Telco Ports, Numbered
* Performance：ISO/IEC-11801
* Ports/IDC Connects ：Nickel and Phosphor Bronze
* Port Identification： Numbered
* Fixings： Supplied M6 Nuts and Bolts

\* Specifications and product design are subject to change. E&OE.